SIP SERVERS:

|  |  |  |
| --- | --- | --- |
| sip.thevoicemanager.com | 65.48.100.36 |  PINGABLE |
| sip2.thevoicemanager.com | 216.86.41.69 |  |

FTP SERVER: (Server address in the phone)

|  |  |  |
| --- | --- | --- |
| ftp.thevoicemanager.com | 65.48.100.98  | NOT PINGABLE |
| USER NAME: |  |  |
| PW: |  |  |

**FUSION360 FIREWALL SETTINGS**

DISABLE ALL VOIP SETTINGS IN THE ROUTER INCLUDING SIP ALG’S.

|  |  |  |
| --- | --- | --- |
| PORT NAME | PROTOCAL | RANGE |
| SIP | TCP/UDP | 5060 |
| RTP | UDP | 10000 - 65000 |

**SPI (Stateful Packet Inspection) --> ( Needs to be disabled )**

**SIP Transformations -->  ( Needs to be disabled )**

**SIP ALG (SIP Application Layer Gateway) --> ( Needs to be disabled )**

**NAT Filtering --> ( Needs to be disabled )**

**SIP Inspection -- >( Needs to be disabled )**